Vastu/Mumbai/01/2024/6211/2304416
09/04-118-JASK
 Date: 09.01.2024

**Structural Stability Report**

Structural Observation Report of Residential Flat No. 204, 2nd Floor, Wing - B, **"Saikrupa Complex Co-op. Hsg. Soc. Ltd."**, Vasant Nagari, Village - Achole, Vasai (East), Taluka - Vasai, District - Palghar, PIN - 401 208, State - Maharashtra, Country - India.

Name of Owner: **Mr. Mahendra Purohit & Mrs. Urmilaben Mahendra Purohit**

This is to certify that on visual inspection, it appears that the structure of the at **“Saikrupa Complex Co-op. Hsg. Soc. Ltd.”**, is in average condition and the future life can be reasonably taken under good condition and with proper periodic repairs & maintenance is about 45 years.

**General Information**:

|  |  |
| --- | --- |
| **A.** | **Introduction** |
| 1 | Name of Building | **“Saikrupa Complex Co-op. Hsg. Soc. Ltd.”** |
| 2 | Property Address | Residential Flat No. 204, 2nd Floor, Wing - B, **"Saikrupa Complex Co-op. Hsg. Soc. Ltd."**, Vasant Nagari, Village - Achole, Vasai (East), Taluka - Vasai, District - Palghar, PIN - 401 208, State – Maharashtra, Country – India. |
| 3 | Type of Building | Residential  |
| 4 | No. of Floors | Ground + 4 Upper Floors |
| 5 | Whether stilt / podium / open parking provided | Open Car Parking Space  |
| 6 | Type of Construction | R.C.C. Framed Structure |
| 7 | Type of Foundation | R.C.C. Footing |
| 8 | Thickness of the External Walls | 9” thick brick walls both sides plastered |
| 9 | Type of Compound | Brick Masonry Walls |
| 10 | Year of Construction | 2008 (as per Part Occupancy Certificate) |
| 11 | Present age of building | 15 Years |
| 12 | Residual age of the building | 45 Years Subject to proper, preventive periodic maintenance & structural repairs. |
| 13 | No. of flats (Per Floor) | 2nd Floor is having 4 Flats |
| 14 | Methodology adopted | As per visual site inspection  |

|  |  |
| --- | --- |
| **B.** | **External Observation of the Building** |
| 1 | Plaster | Good Condition |
| 2 | Chajjas | Good Condition |
| 3 | Plumbing | Good Condition |
| 4 | Cracks on the external walls | Minor cracks found |
| 5 | Filling cracks on the external walls | Found |
| 6 | Cracks on columns & beams | Not found |
| 7 | Vegetation | Not found |
| 8 | Leakages of water in the drainage pipes or water pipes | Not found |
| 9 | Dampness external in the wall due to leakages | Not found  |
| 10 | Any other observation about the condition of external side of the building | 1. **Structural Stability Report from licensed structural engineers not provided for our verification.**
 |
| **C** | **Internal Observation of the common areas of the building and captioned premises** |
| 1 | Beams (Cracks & Leakages) | Not found  |
| 2 | Columns (Cracks & Leakages) | Not found |
| 3 | Ceiling (Cracks & Leakages) | Not found |
| 4 | Leakages inside the property | Not found |
| 5 | Painting inside the property | Good |
| 6 | Maintenance of staircase & cracks | Good |

|  |  |
| --- | --- |
| **D** | **Common Observation** |
| 1 | Structural Audit of the Building Under Bye – Laws No. 77 of the Model Bye Laws (Co-Operative Societies Act / Rules)  | As per bye Laws No. 77 of Co-Op. Societies bye Laws under the Act the society shall conduct a Structural Audit of the building of the society as follows |
| 2 | Remark | No Structural Audit Report is furnished for the perusal.  |

|  |  |
| --- | --- |
| **E** | **Conclusion** |
| The captioned building is having Ground + 4 Upper Floors which are constructed in year 2008 (as per Part Occupancy Certificate). Estimated future life under present circumstances is about 45 years subject to proper, preventive periodic maintenance & structural repairs.The inspection dated 30.11.2023 reveals no structural damage or deterioration to the building. The building is well as the property is maintained in good condition & will stand future life subject to proper, preventive periodic maintenance & Good structural repairs.Our Observations about the structure are given above.The above assessment is based on visual inspection only. Separate structural audit from licensed structural engineers is advised to assess exact balance life of structure.  |

## Sharadkumar B. Chalikwar

Govt. Reg. Valuer

Chartered Engineer (India)

Reg. No. (N) CCIT/1-14/52/2008-09

BOB Empanelment No.: ZO:MZ:ADV:46:941

**Actual Site Photographs**





