Vastu/Mumbai/07/2024/009664/2307063  
03/16-67-PSVS  
 Date: 03.07.2024

**Structural Stability Report**

Structural Observation Report of Residential Flat No. 402, 4th Floor, Building No 30A, **"Bimbisar Nagar Meghdoot Co-Op. Hsg. Soc. Ltd."**, BImbisar Nagar, Western Express Highway, Village - Goregaon, Municipality Ward No. P South, Taluka - Borivali, District - Mumbai Suburban, Goregaon (East), PIN Code - 400 065, State - Maharashtra, Country – India.

Name of Owner: **Shri. Shrikant Sudamrao Galinde**

This is to certify that on visual inspection, it appears that the structure of the at **"Bimbisar Nagar Meghdoot Co-Op. Hsg. Soc. Ltd."**, is in normal condition and the future life can be reasonably taken under good condition and with proper periodic repairs & maintenance is about 39 years.

**General Information**:

|  |  |  |
| --- | --- | --- |
| **A.** | **Introduction** | |
| 1 | Name of Building | **"Bimbisar Nagar Meghdoot Co-Op. Hsg. Soc. Ltd."** |
| 2 | Property Address | Residential Flat No. 402, 4th Floor, Building No 30A, **"Bimbisar Nagar Meghdoot Co-Op. Hsg. Soc. Ltd."**, BImbisar Nagar, Western Express Highway, Village - Goregaon, Municipality Ward No. P South, Taluka - Borivali, District - Mumbai Suburban, Goregaon (East), PIN Code - 400 065, State - Maharashtra, Country - India. |
| 3 | Type of Building | Residential used |
| 4 | No. of Floors | Stilt + 7th Upper Floors |
| 5 | Whether stilt / podium / open parking provided | Stilt Parking |
| 6 | Type of Construction | R.C.C. Framed Structure |
| 7 | Type of Foundation | R.C.C. Footing |
| 8 | Thickness of the External Walls | 9” thick brick walls both sides plastered |
| 9 | Type of Compound | Brick Masonry Walls |
| 10 | Year of Construction | 2003 (As per occupancy certificate) |
| 11 | Present age of building | 21 years |
| 12 | Residual age of the building | 39 years Subject to proper, preventive periodic maintenance & structural repairs. |
| 13 | No. of flats (Per Floor) | 04 Flats on 4th Floor |
| 14 | Methodology adopted | As per visual site inspection |

|  |  |  |
| --- | --- | --- |
| **B.** | **External Observation of the Building** | |
| 1 | Plaster | Normal Condition |
| 2 | Chajjas | Normal Condition |
| 3 | Plumbing | Normal Condition |
| 4 | Cracks on the external walls | Minor cracks found |
| 5 | Filling cracks on the external walls | Not found |
| 6 | Cracks on columns & beams | Minor cracks found |
| 7 | Vegetation | Not Found |
| 8 | Leakages of water in the drainage pipes or water pipes | Not Found |
| 9 | Dampness external in the wall due to leakages | Not Found |
| 10 | Any other observation about the condition of external side of the building | Structural Stability Report from licensed structural engineers not provided for our verification. |
| **C** | **Internal Observation of the common areas of the building and captioned premises** | |
| 1 | Beams (Cracks & Leakages) | Minor cracks and leakages found |
| 2 | Columns (Cracks & Leakages) | Minor cracks found |
| 3 | Ceiling (Cracks & Leakages) | Minor cracks found |
| 4 | Leakages inside the property | Not Found |
| 5 | Painting inside the property | Good Condition |
| 6 | Maintenance of staircase & cracks | Normal |

|  |  |  |
| --- | --- | --- |
| **D** | **Common Observation** | |
| 1 | Structural Audit of the Building Under Bye – Laws No. 77 of the Model Bye Laws (Co-Operative Societies Act / Rules) | As per bye Laws No. 77 of Co-Op. Societies bye Laws under the Act the society shall conduct a Structural Audit of the building of the society as follows |
| 2 | Remark | No Structural Audit Report is furnished for the perusal. |

|  |  |
| --- | --- |
| **E** | **Conclusion** |
| The captioned building is having Stilt + 7th Upper Floors which are constructed in year 2003 (As per occupancy certificate). Estimated future life under present circumstances is about 39 years subject to proper, preventive periodic maintenance & structural repairs.  The inspection dated 02.07.2024 of building. The building is well as the property is maintained in normal condition & will stand future life subject to proper, preventive periodic maintenance & Good structural repairs.  Our Observations about the structure are given above.  The above assessment is based on visual inspection only. Separate structural audit from licensed structural engineers is advised to assess exact balance life of structure. | |

## Sharadkumar B. Chalikwar

Structural Engineer Licence No. STATE/R/2022/APL/01785

Govt. Reg. Valuer

Chartered Engineer (India)

Reg No. (N) CCIT/1-14/52/2008-09

SBI Empanelment No.: SME / TCC / 38 / 37

**Actual site photographs**







**Actual site photographs**



