Vastu/Mumbai/08/2024/010555/2307819  
23/07-297-PRSK  
 Date: 22.08.2024

**Structural Stability Report**

Structural Observation Report of Residential Flat No. 12, 2nd Floor, **"Vasant Vihar Co-Op. Hsg. Soc. Ltd. ",** Plot No. 17, New Nagardas Cross Road, Village - Andheri, Andheri (East), Mumbai - 400 069, State - Maharashtra, Country - India.

Name of Owner: **Mr. Kamabhai Jivraj Solanki, Mr. Chetan Kamabhai Solanki & Mrs. Kanta Kamabhai Solanki**

This is to certify that on visual inspection, it appears that the structure of the at **" Vasant Vihar Co-Op. Hsg. Soc. Ltd."**, is in normal condition and the future life can be reasonably taken under good condition and with proper periodic repairs & maintenance is about 45 years.

**General Information**:

|  |  |  |
| --- | --- | --- |
| **A.** | **Introduction** | |
| 1 | Name of Building | **"Vasant Vihar Co-Op. Hsg. Soc. Ltd."** |
| 2 | Property Address | Residential Flat No. 12, 2nd Floor, **"Vasant Vihar Co-Op. Hsg. Soc. Ltd. ",** Plot No. 17, New Nagardas Cross Road, Village - Andheri, Andheri (East), Mumbai - 400 069, State - Maharashtra, Country - India |
| 3 | Type of Building | Residential used |
| 4 | No. of Floors | Ground + 6th Upper Floors |
| 5 | Whether stilt / podium / open parking provided | Open Car Parking Space |
| 6 | Type of Construction | R.C.C. Framed Structure |
| 7 | Type of Foundation | R.C.C. Footing |
| 8 | Thickness of the External Walls | 9” thick brick walls both sides plastered |
| 9 | Type of Compound | Brick Masonry Walls |
| 10 | Year of Construction | 2005 (As per site information) |
| 11 | Present age of building | 19 years |
| 12 | Residual age of the building | 41 years Subject to proper, preventive periodic maintenance & structural repairs. |
| 13 | No. of flats (Per Floor) | 04 Flats on 2nd Floor |
| 14 | Methodology adopted | As per visual site inspection |

|  |  |  |
| --- | --- | --- |
| **B.** | **External Observation of the Building** | |
| 1 | Plaster | Normal Condition |
| 2 | Chajjas | Normal Condition |
| 3 | Plumbing | Normal Condition |
| 4 | Cracks on the external walls | Not Found |
| 5 | Filling cracks on the external walls | Not Found |
| 6 | Cracks on columns & beams | Not Found |
| 7 | Vegetation | Not Found |
| 8 | Leakages of water in the drainage pipes or water pipes | Not Found |
| 9 | Dampness external in the wall due to leakages | Not Found |
| 10 | Any other observation about the condition of external side of the building | Structural Stability Report from licensed structural engineers not provided for our verification. |
| **C** | **Internal Observation of the common areas of the building and captioned premises** | |
| 1 | Beams (Cracks & Leakages) | Not Found |
| 2 | Columns (Cracks & Leakages) | Not Found |
| 3 | Ceiling (Cracks & Leakages) | Not Found |
| 4 | Leakages inside the property | Not Found |
| 5 | Painting inside the property | Normal Condition |
| 6 | Maintenance of staircase & cracks | Good |

|  |  |  |
| --- | --- | --- |
| **D** | **Common Observation** | |
| 1 | Structural Audit of the Building Under Bye – Laws No. 77 of the Model Bye Laws (Co-Operative Societies Act / Rules) | As per bye Laws No. 77 of Co-Op. Societies bye Laws under the Act the society shall conduct a Structural Audit of the building of the society as follows |
| 2 | Remark | No Structural Audit Report is furnished for the perusal. |

|  |  |
| --- | --- |
| **E** | **Conclusion** |
| The captioned building is having Ground + 6th Upper Floors which are constructed in year 2005 (As per site information) Estimated future life under present circumstances is about 41 years subject to proper, preventive periodic maintenance & structural repairs.  The inspection dated 16.08.2024 of building. The building is well as the property is maintained in normal condition & will stand future life subject to proper, preventive periodic maintenance & Good structural repairs.  Our Observations about the structure are given above.  The above assessment is based on visual inspection only. Separate structural audit from licensed structural engineers is advised to assess exact balance life of structure. | |

## Sharadkumar B. Chalikwar

Structural Engineer Licence No. STATE/R/2022/APL/01785

Govt. Reg. Valuer

Chartered Engineer (India)

Reg No. (N) CCIT/1-14/52/2008-09

**Actual site photographs**



